Sense the paper through IR sensor

True False

Moves to folding mechanism

Glue flow stops

Glue flows through funnel on the paper

Roller start rotating through DC motor

Paper moves to gluing section

Sense the paper

Servo motor rotates 90 to 0 degree and remains till paper is not sensed

Servo motor rotates 0 to 90 degree and remains till the paper sensed

Roller stops rotating